DTC DETECTION LOGIC NOTE：

- If DTC B2605 is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.
- If DTC B2605 is displayed with DTC U1010, first perform the trouble diagnosis for DTC U1010. Refer to DTC Logic.
- If DTC B2605 is displayed with DTC U1010, first perform the trouble diagnosis for DTC B2603. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2605 | PNP SW | BCM detects the following status for 500 ms or more when the ignition switch is in ON position

- N position input signal exists. Shift position signal from IPDM E/R does not exist.
- N position input signal does not exist. Shift position signal from IPDM E/R exists.

- Harness or connectors
  [TCM circuit is open or shorted]
- BCM
- IPDM E/R
- TCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn ignition switch ON under the following conditions and wait for at least 1 second.

- Shift lever is in the P or N position
- Do not depress the brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END