1.CHECK SET-UP SWITCH (VDC)

1. Turn the ignition switch OFF.
2. Disconnect set-up switch (VDC) harness connector.
3. Check the continuity between set-up switch (VDC) harness connector terminals.

   Set-up switch (VDC) | Condition | Continuity
   Terminal
   12 – 17 | When the set-up switch (VDC) is operated upward | Not existed
   When the set-up switch (VDC) is operated downward | Existed
   5 – 17 | When the set-up switch (VDC) is operated upward | Existed
   When the set-up switch (VDC) is operated downward | Not existed
   1 – 18 | — | Existed
   3 – 18 | — | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace set-up switch (VDC). Refer to Exploded View.