REMOVAL

1.Remove instrument lower panel (driver). Refer to Exploded View.

2.Remove the footrest. Refer to Exploded View.

3.Remove the kicking plate inner, dash side finisher and floor trim. Refer to Exploded View.

4.Disconnect the harness connectors of ASCD brake switch and stop lamp switch.

5.Rotate ASCD brake switch and stop lamp switch counterclockwise to remove.

6.Remove the snap pin, and then remove the clevis pin from the clevis of brake booster.

7.Remove the brake pedal assembly.

INSTALLATION
Install in the reverse order of removal.