INITIALIZATION PROCEDURE ■ CAUTION ■ If the initialization is not complete, UP does not operate while door is open.

1.Disconnect the battery negative terminal or power window motor connector, and then reconnect.

2.Door close (door switch OFF).

3.Turn ignition switch ON.

4.Operate power window switch to open the glass halfway or more. (This operation is not necessary if the glass is already open halfway or more)

5.Continue pulling power window switch UP (AUTO UP operation). Even after the glass stops at the fully open position, continue pulling the switch for 3 seconds or more.

6.Check anti-pinch function.

NOTE：
The work procedures for driver seat and passenger seat are the same.
CHECK ANTI-PINCH FUNCTION

1.Fully open the door window.

2.Place a piece of wood near the fully closed position.

3.Close door glass completely using AUTO UP.

- Check that glass starts to lower without pinching the piece of wood, lowers approximately 150 mm, and then stops. When the piece of wood is 60 mm thick or more, glass may lower approximately 100 mm and then stop.
- Check that glass does not rise when operating the power window main switch while lowering.

■ CAUTION ■

- Never check with hands or other body parfs because they may be pinched. Never get pinched.
- Check that AUTO UP operation before inspection during system initialization is performed.
- It may switch to fail-safe mode if open/close operation is performed continuously. Perform initial setting in that situation. Refer to Fail-Safe
- Perform initial setting when AUTO UP operation or anti-pinch function does not operate normally.
- Finish initial setting. Otherwise, the next operation cannot be done.

1. AUTO UP operation
2. Anti-pinch function
3. Automatic window adjusting function
4. Retained power operation