THIS OCCUPANT CLASSIFICATION SYSTEM HAS THE FOLLOWING FUNCTION.

- Suppress the deployment of front passenger air bag when front passenger seat is empty, or when occupied by child and child-seat. Turns on front passenger air bag OFF indicator when front passenger seat is occupied by child-seat and child.
- Indicates malfunction portion with blinking times of air bag warning lamp in diagnosis mode.
- Indicates the malfunctioning record by CONSULT-III.

NOTE：
Operation of air bag diagnosis sensor unit when air bag diagnosis sensor unit receives information from Occupant Classification System

Status (front passenger seat) | Passenger air bag | Front passenger air bag OFF indicator | Air bag warning lamp | Seat belt warning lamp (when front passenger seat is unbuckled)
Empty | Suppress | OFF | OFF | OFF
Child/ child-seat | Suppress | ON | OFF | ON
Adult | Enable to deploy | OFF | OFF | ON
Malfunction | Suppress | ON | Blinking | OFF