REMOVAL

1.Remove the trunk rear finisher. Refer to Exploded View.

2.Remove the mounting bolts, and then remove the trunk lid striker.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Apply anticorrosive agent onto the mounting surface.
- After installation, perform the fitting adjustment. Refer to Adjustment.
- After installation, check trunk lid open/close, lock/unlock operation.