INSPECTION AFTER REMOVAL Check the following items and replace the brake pedal assembly if necessary.

- Check the brake pedal for bend, damage, or cracks on the welded parts.
- Check clevis pin and plastic stopper (A) for damage or deformation. If any damage is found, replace clevis pin.

ADJUSTMENT AFTER INSTALLATION

- Adjust each item of brake pedal after installing the brake pedal assembly to the vehicle. Refer to Inspection and Adjustment.
- Perform the release position learning of the accelerator pedal. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).