1.Remove filler plug (1). Fill up with new gear oil until oil level reaches the specified level (A).

Oil grade and Viscosity | : Refer to Fluids and Lubricants.
Oil capacity | : Refer to General Specifications.

2.After refilling oil, check oil level. Set a gasket to filler plug (1), and then install it to final drive and tighten to the specified torque.

Standard |
Filler plug tightening torque | : 34.5 N·m (3.5 kg-m, 25 ft‐lb)

■ CAUTION ■
Never reuse gasket.