REMOVAL

1.Remove the mounting clips and the double-faced adhesive tape of the body side weather-strip.

2.Remove the body side weather-strip.
NOTE：
Disengage the joint of front pillar clip while sliding upward.

3.Remove the mounting screws (A) and the clip (B), and then remove the weather-strip retainer (1).

4.Insert the remover tool (A) from the rear edge of the front pillar finisher (1), and then disengage the clips toward vehicle front.
■ CAUTION ■
Apply protective tape (B) to the body side to protect from damage.

| : Clip

5.Remove the front door finisher from the vehicle body.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- During installation check that the clips are aligned with the vehicle body side panel holes, and then press.
- Never reuse the body side weather-strip.
- To maintain adhesion, never wash the vehicle within 24 hours after installing the body side weather-strip.