1.CHECK AXIS B FEED PRESSURE SOLENOID VALVE CIRCUIT Refer to Diagnosis Procedure (NHPC). Is the inspection result normal? YES >>GO TO 2. NO >>Repair or replace damaged parts.
2.CHECK CLUTCH B SOLENOID VALVE CIRCUIT
Refer to Diagnosis Procedure (NHPC).
Is the inspection result normal?
YES >>GO TO 3.
NO >>Repair or replace damaged parts.
3.CHECK CLUTCH B PRESSURE SENSOR CIRCUIT
Refer to Diagnosis Procedure (NHPC) and Diagnosis Procedure (NHPC).
Is the inspection result normal?
YES >>GO TO 4.
NO >>Repair or replace damaged parts.
4.CHECK GROUND CONNECTION

1. Turn ignition switch OFF.
2. Check ground connections B31 and ground cable connections. Refer to “Ground Inspection” in Circuit Inspection.

Is the inspection result normal?
YES >>GO TO 5.
NO >>Repair or replace damaged parts.
5.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
Is the inspection result normal?
YES >>Replace transmission assembly. Refer to Exploded View (GT-R certified NISSAN dealer).
NO >>Repair or replace damaged parts.