■ CAUTION ■

- Disconnect the battery negative terminal or remove the fuse.
- Never touch the glass of bulb directly by hand. Keep grease and other oily matters away from it.
- Never touch bulb by hand while it is lit or right after being turned off.
- Never leave bulb out of lamp reflector for a long time because dust, moisture smoke, etc. may affect the performance of lamp. When replacing bulb, be sure to replace it with new one.

REAR TURN SIGNAL LAMP BULB

1.Remove the trunk lid finisher. Refer to Exploded View.

2.Remove the rubber cover (1).

3.Turn the rear turn signal lamp bulb socket (2) counterclockwise and unlock it.

4.Remove the bulb (3) from the rear turn signal lamp bulb socket.

BACK-UP LAMP BULB

1.Remove the trunk lid finisher. Refer to Exploded View.

2.Remove the rubber cover (1).

3.Turn the back-up lamp bulb socket (2) counterclockwise and unlock it.

4.Remove the bulb (3) from the back-up lamp bulb socket.