INSPECTION AFTER INSTALLATION

- Check for fluid leakage from connections, damage, twists, deformation or contact with other parts. Replace if necessary.
  ■ CAUTION ■
  If the looseness of connection or fluid leakage is present, retighten to the specified torque. Replace if necessary.
- Depress the brake pedal with a force of 785 N (80 kg, 176 lb) and hold down the pedal for approximately 5 seconds with the engine running. Check for any fluid leakage.