REMOVAL

1.Remove driver seat. Refer to Exploded View.

2.Remove the rear side finisher. Refer to Exploded View.

3.Remove the dash side finisher (RH). Refer to Exploded View.

4.Remove floor carpet hook. Refer to Exploded View.

5.Remove the front seat belt (RH) anchor bolt. Refer to Exploded View.

6.Pull up the floor carpet and remove the floor spacer.
■ CAUTION ■

- Never damage the floor spacer.

- Never apply excessive force against the floor carpet.

7.Disconnect AWD control unit harness connector.

8.Remove the bolts () from AWD control unit (1).

9.Remove AWD control unit.

INSTALLATION
Installation is the reverse order of removal.