1.CHECK FUSES Check that the following fuses are not blown:

Power source | Fuse No.
Battery | 11
Ignition switch ON or START | 4

Is the inspection result normal?
YES>>GO TO 2.
NO>>Replace the fuse with a new one after repairing the applicable circuit.
2.CHECK POWER SUPPLY CIRCUIT
Check the voltage between the combination meter harness connector terminals and the ground.

Terminal No. | Signal name | Ignition switch | Voltage
1 | Battery power supply | OFF | Battery voltage
2 | Ignition signal | ON | Battery voltage

Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair the harness between the fuse and the combination meter.
3.CHECK GROUND CIRCUIT

1. Turn the ignition switch OFF.
2. Disconnect the combination meter connector.
3. Check for continuity between the combination meter harness connector terminals and the ground.

   Combination meter | Ground | Continuity
   Connector | Terminal
   M53 | 3 | Existed
   5

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair the harnesses or connectors.