1.CHECK SET-UP SWITCH (VDC) 1 Check that the R mode indicator lamp (next to the switch) illuminates when pulling up the set-up switch (VDC) for approximately 1 second or more. Is the inspection result normal? YES>>GO TO 2. NO>>Check the set-up switch (VDC). Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
2.CHECK SET-UP SWITCH (VDC) 2
Check that the OFF mode indicator lamp (next to the switch) illuminates when pushing down the set-up switch (VDC) for approximately 1 second or more.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Check the set-up switch (VDC). Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
3.CHECK SET-UP SWITCH (VDC) 3
Check that the VDC OFF indicator lamp in the combination meter illuminates when pushing down the set-up switch (VDC) for approximately 1 second or more.
Is the inspection result normal?
YES>>INSPECTION END
NO>>Check the set-up switch (VDC). Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).