REMOVAL

1.Use a refrigerant collecting equipment (for HFC‐134a) to discharge the refrigerant.

2.Remove air intake duct assembly 1 together with charge air cooler. Refer to Exploded View (GT-R certified NISSAN dealer).

3.Clean liquid tank and its surrounding area, and then remove dust and rust from liquid tank.
■ CAUTION ■
Be sure to clean carefully.

4.Remove mounting bolts of liquid tank bracket.

5.Remove mounting bolts of liquid tank, and then remove liquid tank from condenser.
■ CAUTION ■
Cap or wrap the joint of the cooler piping and liquid tank with suitable material such as vinyl tape to avoid the entry of air.

INSTALLATION
Install liquid tank, and then install liquid tank bracket on condenser.
■ CAUTION ■

- Check that liquid tank bracket is securely installed at protrusion of condenser. (Check that liquid tank bracket does not move to a position below center of liquid tank.)
- Replace O‐rings of the cooler piping with new ones. Then apply compressor oil to them when installing.
- Check for leakages when recharging refrigerant.