REMOVAL

1.Disengage the clips, and then remove the radiator cover.

2.Remove the front bumper fascia and the bumper reinforcement. Refer to Removal and Installation.

3.Remove the dust duct side (LH/RH). Refer to Exploded View.

4.Remove the harness clip and hood lock cable clamp from the bumper fascia bracket.

5.Remove the hood lock cable clamp from the air intake duct assembly 1.

6.Disengage the connector of horns (HIGH/LOW). Refer to Removal and Installation.

7.Disengage the hood switch connector of hood lock (RH).

8.Disconnect the ambient sensor connector. Refer to Exploded View.

9.Remove the power steering oil cooler mounting bolt. Refer to Exploded View.

10.Remove the washer tank and the washer tank inlet. Refer to Exploded View.

11.Disconnect the air inlet hose, air inlet pipe, and recirculation hose from the charge air cooler assembly (bank 1 and bank 2). Refer to Exploded View.

12.Remove the mounting bolts of charge air cooler assembly [bank 1: (1), bank 2: (2)] by the arrows in the figure.

13.Remove the mounting bolts of the hood lock (LH/RH).

14.Check that all connections of connector, hose, and pipe are disconnected from the air intake duct assembly.

15.Remove the mounting bolts, and then remove the air intake duct assembly.

16.Remove the hood lock (LH/RH) from the air intake duct assembly 1.

17.Remove the hood lock control cable (front) from the hood lock (LH/RH).

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- After installation, check hood open/close, lock/unlock operation.
- After installation, perform the fitting adjustment. Refer to Adjustment.