■ WARNING ■ Be sure to read “General Precautions” when working on the fuel system. Refer to General Precautions (GT-R certified NISSAN dealer). REMOVAL

- Drain fuel from fuel tank if necessary. Refer to Removal and Installation (GT-R certified NISSAN dealer).
- Perform work on level place.

1.Perform steps 2 to 7 of “REMOVAL” in “ FUEL LEVEL SENSOR UNIT, FUEL FILTER AND FUEL PUMP ASSEMBLY” on main and sub fuel level sensor units. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Remove exhaust sub muffler and main muffler assembly. Refer to Exploded View.

3.Separate main propeller shaft and front propeller shaft. Refer to Exploded View and Exploded View.

4.Remove transmission and rear suspension member assembly. Refer to Exploded View.
NOTE：
For this service, drive shaft, transmission, and rear suspension member are required not to be separate one another during removal.

5.Disconnect EVAP hose (1), vent hose (2), and fuel filler hose (3) at fuel tank side.

A | : Vehicle left side
B | : Vehicle right side
| : Vehicle front

- To disconnect quick connector, refer to Removal and Installation (GT-R certified NISSAN dealer).

6.Remove fuel tank protector.

7.Support the lower part of fuel tank (1) using transmission jack (A).
■ CAUTION ■
To secure the support, place wooden blocks or something at the position where fuel tank mounting bands never engage.

8.Remove fuel tank mounting bands.

9.Remove fuel tank mounting bolts and nuts.

10.Supporting fuel tank with hands, descend transmission jack carefully, and remove fuel tank.
■ CAUTION ■

- Check that all connection points are disconnected.
- Check that there is no interference with vehicle.

11.Remove fuel filler tube if necessary.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Insert hose to the length specified below and fix it by hose clamp.

  Fuel filler hose | : 35 mm (1.38 in)
  The other hoses | : 25 mm (0.98 in)

- Check that hose clamp is not placed on swelled area of fuel tube.
- Tighten the clamp band with the top mark (A) until the mark is on the bolt head flange.
- To connect quick connector, refer to Removal and Installation (GT-R certified NISSAN dealer).