REMOVAL

1.Use a refrigerant collecting equipment (for HFC-134a) to discharge the refrigerant.

2.Remove air intake duct assembly 1 together with charge air cooler. Refer to Exploded View (GT-R certified NISSAN dealer).

3.Disconnect one-touch joint between high‐pressure flexible hose and condenser with disconnector (SST: 9253089912). Refer to Exploded View (GT-R certified NISSAN dealer).

4.Disconnect one-touch joint between high‐pressure pipe 1 and condenser with disconnector (SST: 9253089908). Refer to Exploded View (GT-R certified NISSAN dealer).

5.Remove mounting bolts (upper side), and then remove condenser.

INSTALLATION
Installation is basically the reverse order of removal.
■ CAUTION ■

- Replace O‐rings with new ones. Then apply compressor oil to them when installing.
- Female‐side piping connection is thin and easy to deform. Slowly insert the male‐side piping straight in axial direction.
- Insert piping securely until a click is heard.
- After piping connection is completed, pull male‐side piping by hand to make sure that connection does not come loose.
- Check for leakages when recharging refrigerant.