| Capacity (Approximate) | Recommended Fluids/Lubricants
US measure | Imp measure | Liter
Engine oil Drain and refill | With oil filter change | 5-3/4 qt | 4-7/8 qt | 5.5 | Mobil 1 (0W-40)*1
Without oil filter change | 5-1/4 qt | 4-3/8 qt | 5.0
Dry engine (Overhaul) | 7-1/8 qt | 5-7/8 qt | 6.7
Cooling system | With reservoir tank | 11-5/8 qt | 9-5/8 qt | 11.0 | Genuine NISSAN Long Life Antifreeze/ Coolant (blue) or equivalent
Reservoir tank | 1-1/2 qt | 1-1/4 qt | 1.4
Transmission oil*5 | 10-1/4 qt | 8-1/2 qt | 9.7 | Genuine NISSAN Transmission Oil R35 Special*2
Differential gear oil | Front | 1-3/8 pt | 1-1/8 pt | 0.65 | Castrol SAF-XJ 75W-140*2
Rear | 3-1/4 pt | 2-3/4 pt | 1.55
Transfer fluid | — | — | — | —
Power steering fluid (PSF) | 1-1/8 qt | 7/8 qt | 1.0 | Genuine NISSAN PSF or equivalent*3
Brake fluid | — | — | — | Genuine NISSAN Brake Fluid R35 Special II*4
Multi-purpose grease | — | — | — | NLGI No. 2 (Lithium soap base)
Windshield washer fluid | — | — | — | Genuine NISSAN Windshield Washer Concentrate Cleaner & Antifreeze or equivalent
Fuel recommendation | — | — | — | Refer to Fuel.
*1: Mobil 1 (0W-40) (100% synthetic) is the factory fill oil. The VR38 engine with its plasma-sprayed bores was developed using this oil. NISSAN cannot ensure proper engine operation and durability if other 0W-40 synthetic oil is used. If Mobil 1 (0W-40) is not available, Mobil 1 (10W-40) (100% synthetic) may be used; however, some performance loss may be noticed. For further details, see “Engine Oil Recommendation”.
*2: The use of fluids and lubricants other than the specified may cause vehicle malfunctions and result in non-warranty vehicle repairs.
*3: DEXRON™ VI type ATF or Canada NISSAN Automatic Transmission Fluid may also be used.
*4: Genuine NISSAN Brake Fluid R35 Special II is the factory fill brake fluid. The Vehicle Dynamic Control (VDC) unit and other related parts were specially designed for this brake fluid and NISSAN cannot ensure the best performance and proper operation of the vehicle if other brake fluid is used.
*5: All of the fluid cannot be removed when servicing the transmission. The actual refill amount may be less than shown.