DISASSEMBLY ■ CAUTION ■ Always shift the shift lever in the N position when performing disassembly and assembly of A/T shift selector assembly.

1.Press the shift lock release button, and then shift the shift lever in the N position.

2.Insert a flat-bladed screwdriver into tabs (A: 4 locations), and remove the position indicator plate (1) from the A/T shift selector assembly (2) while lifting it up.
■ CAUTION ■
The tabs crack easily. Be careful when removing.

3.Remove the starter switch from the position indicator plate.

4.Remove the slide cover from the A/T shift selector assembly.

Assembly
Note the following, and assemble in the reverse order of disassembly.

- Align the convex area (A) of slide cover (1) with the convex area (B) of A/T shift selector assembly (2) as shown in the figure, and then install the position indicator plate. Check the shift lever movement after installation. Assemble again if any malfunctioning condition is detected.