REMOVAL

1.Remove the door finisher. Refer to Removal and Installation.

2.Fully close the door window.

3.Remove the door speaker.

4.Remove the door check link (body side) mounting bolts.

5.Remove the driver side mounting bolts of door check link, and then remove the door check link from the inside of the door panel.
■ CAUTION ■
Never damage the door window with the door check link.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Apply anticorrosive agent onto the mounting surface.
- After installation, check door open/close operation.