CONSULT‐III can perform the following diagnosis modes by the CAN communication with combination meter.

Diagnosis mode | Description
Self Diagnosis Result | Displays names of malfunctioning systems judged by and stored in combination meter.
Data Monitor | Displays combination meter input/output data in real time.
Special function | Displays the illumination record of warning lamp and indicator lamp.

SELF DIAGNOSTIC RESULT
NOTE：
Details of time display

- CRNT: Displays during the current malfunctioning detection.
- PAST: Displays if any previous malfunction is present when the current status is normal.

IGN counter

- The IGN counter is displayed on the freeze frame data (FFD).
- The IGN counter indicates the number of times ignition switch is turned ON after the DTC detection.

- The number is 0 when a malfunction is detected now.
- The number increases like 1 → 2 → 3 → ... 38 → 39 after returning to the normal condition whenever the ignition switch is turned OFF → ON.
- The number is fixed to 39 unit the self-diagnosis results are erased if it is over 39.

Display contents of CONSULT-III | Diagnostic item is detected if ...
CAN COMM CIRCUIT [U1000] | Combination meter cannot communicate CAN communication signal for 2 seconds or more.
CONTROL UNIT (CAN) [U1010] | Malfunction is detected during initial diagnosis of combination meter CAN controller.
VEHICLE SPEED [B2205] | Abnormal vehicle speed signal is received from ABS actuator and electric unit (control unit).
ENGINE SPEED [B2267] | ECM continuously transmits abnormal engine speed signal for 2 seconds or more.
WATER TEMP [B2268] | ECM continuously transmits abnormal engine coolant temperature signal for 60 seconds or more.
OIL LEV SEN OPEN [B2321] | Signal from oil level sensor is broken (resistance value of oil level sensor exceeds 20 Ω).
OIL LEV SEN SHORT [B2322] | Signal from oil level sensor is shorted (resistance value of oil level sensor is less than 3 Ω).

DATA MONITOR

Monitor item | MAIN ITEMS | Description
SPEED METER [km/h] | X | Vehicle speed signal value received from ABS actuator and electric unit (control unit) via CAN communication. NOTE： 655.35 is displayed when the malfunction signal is received.
SPEED OUTPUT [km/h] | X | Vehicle speed signal value transmitted to other units via CAN communication. NOTE： 655.35 is displayed when the malfunction signal is received.
ODO OUTPUT [km] |  | Odometer value transmitted to other units via CAN communication.
TACHO METER [rpm] | X | Engine speed signal value received from ECM via CAN communication. NOTE： 8191.875 is displayed when the malfunction signal is received.
FUEL METER [L] | X | Fuel level value indicated on combination meter.
W TEMP METER [°C] | X | Engine coolant temperature signal value received from ECM via CAN communication. NOTE： 215 is displayed when the malfunction signal is received.
ABS W/L [On/Off] |  | ABS warning lamp status judged by the ABS malfunction signal received from ABS actuator and electric unit (control unit) via CAN communication.
VDC/TCS IND [On/Off] |  | VDC OFF indicator lamp status judged by the VDC OFF indicator lamp signal received from ABS actuator and electric unit (control unit) via CAN communication.
SLIP IND [On/Off] |  | SLIP indicator lamp status judged by the SLIP indicator lamp signal received from ABS actuator and electric unit (control unit) via CAN communication.
BRAKE W/L [On/Off] |  | Brake warning lamp status judged by the brake warning lamp signal received from ABS actuator and electric unit (control unit) via CAN communication. NOTE： OFF is displayed when the bulb check is operating, when the brake fluid level switch is ON, or when the brake warning lamp is illuminated when the parking brake switch is ON or the brake fluid level switch is ON during the bulb check operation.
DOOR W/L [On/Off] |  | Door open warning status judged by the door switch signal received from BCM via CAN communication.
HI-BEAM IND [On/Off] |  | High beam indicator lamp status judged by the high beam request signal received from BCM via CAN communication.
TURN IND [On/Off] |  | Turn signal indicator lamp status judged by the turn indicator signal received from BCM via CAN communication.
RR FOG IND [Off] |  | NOTE： This Item is displayed, but cannot be monitored.
OIL W/L [On/Off] |  | Oil pressure warning lamp status judged by the oil pressure sensor signal received from oil pressure sensor.
LIGHT IND [On/Off] |  | Tail lamp indicator lamp status judged by the tail lamp request signal received from BCM via CAN communication.
MIL [On/Off] |  | MIL status judged by the malfunction indicator lamp received from ECM via CAN communication.
CRUISE IND [On/Off] |  | CRUISE indicator lamp status judged by the ASCD status signal received from ECM via CAN communication.
SET IND [On/Off] |  | SET indicator lamp status judged by the ASCD status signal received from ECM via CAN communication.
ATC/T-AMT W/L [On/Off] |  | Transmission check warning lamp status judged by the transmission warning light signal received from TCM via CAN communication.
4WD W/L [On/Off] |  | AWD warning lamp status judged by the AWD warning lamp signal received from AWD control unit via CAN communication.
FUEL W/L [On/Off] |  | Low fuel warning status judged by the fuel level sensor signal received from fuel level sensor unit.
WASHER W/L [On/Off] |  | Low washer fluid warning status judged by the washer level switch signal received from washer level switch.
AIR PRES W/L [On/Off] |  | Tire pressure warning lamp status judged by the tire pressure warning lamp signal received from low tire pressure warning control unit via CAN communication.
KEY G/Y W/L [On/Off] |  | KEY warning lamp (green/yellow) status judged by the KEY warning lamp signal received from BCM via CAN communication.
LCD [B&P N, B&P I, ID NG, ROTAT, SFT P, INSRT, BATT, NO KY, OUTKY, LK WN] |  | Displays status of Intelligent Key system warning detected from meter display signal is received from BCM via CAN communication.
SHIFT IND [P/R/N/A1/A2/A3/A4/A5/A6/M1/M2/M3/M4/M5/M6] |  | Shift position status judged by the shift position signal received from TCM via CAN communication.
PKB SW [On/Off] |  | Parking brake switch status judged by the parking brake switch signal received from parking brake switch.
BUCKLE SW [On/Off] |  | Seat belt buckle switch (driver side) status judged by the seat belt buckle switch signal (driver side) received from seat belt buckle switch (driver side).
BRAKE OIL SW [On/Off] |  | Brake fluid level switch status judged by the brake fluid level switch signal received from brake fluid level switch.
A/C AMP CONN [On/Off] |  | A/C auto amp. connection recognition status judged by the A/C auto amp. connection recognition signal received from A/C auto amp.
ENTER SW [On/Off] |  | Enter switch status judged by the enter switch signal received from meter control switch.
SELECT SW [On/Off] |  | Select switch status judged by the select switch signal received from meter control switch.
DISTANCE [km] |  | Possible driving distance value judged by combination meter.
OUTSIDE TEMP [°C] |  | Ambient sensor value converted from ambient sensor signal received from ambient sensor. NOTE： This may not match the temperature value indicated on information display. (Because the information display value is a corrected value from the ambient sensor input value.)
FUEL LOW SIG [On/Off] |  | Low fuel warning signal status that is output to AV control unit via CAN communication.
CRANKING SIG [On/Off] |  | Cranking status judged by the engine status signal received from ECM via CAN communication.
ST CNT SIG [On/Off] |  | Starter relay status judged by the starter relay status signal received from BCM via CAN communication.
BUZZER [On/Off] | X | Status of buzzer integrated in combination meter judged with buzzer output signal received from each unit via CAN communication and with warning output condition of combination meter.
ENG OIL TMP [°C] |  | Engine oil temperature status judged by the engine oil temperature signal received from ECM via CAN communication.
ENG OIL PRESS [MPa] |  | Engine oil pressure value judged by the oil pressure sensor signal received from oil pressure sensor.
TM OIL TMP [°C] |  | Transmission oil temperature value judged by the transmission oil temperature signal received from TCM via CAN communication.
TM OIL PRESS [MPa] |  | Transmission oil pressure value judged by the transmission oil pressure signal received from TCM via CAN communication.
A/F RATIO |  | Air-fuel ratio value judged by the air-fuel ratio signal received from ECM via CAN communication.
BOOST PRESS [kPa] |  | Boost pressure value judged by the boost pressure signal received from ECM via CAN communication.
THRTL POSI [%] |  | Throttle position value judged by the throttle position signal received from ECM via CAN communication.
TRQ DSTRBT [%] |  | Front torque distribution rate value judged by the front torque distribution rate signal received from AWD control unit via CAN communication.
AMT P SFT [On/Off] |  | P engagement warning display status judged by the shift lever position check display signal received from TCM via CAN communication.
AMT SYS CHCK |  | Transmission system check display status judged by the transmission system check display signal received from TCM via CAN communication.
AMT SFT POSI [On/Off] |  | Shift lever position warning display status judged by the shift lever position warning display signal received from TCM via CAN communication.
AMT OIL TMP H [On/Off] |  | Transmission oil high temperature warning display status judged by the transmission oil high temperature warning display signal received from TCM via CAN communication.
AMT CL TMP H [On/Off] |  | Transmission clutch high temperature warning display status judged by the transmission clutch high temperature warning display signal received from TCM via CAN communication.
AMT CHCK [Off] |  | NOTE： This Item is displayed, but cannot be monitored.
AMT MALF [On/Off] |  | Transmission system warning display status judged by the transmission system warning display signal received from TCM via CAN communication.
TPMS FLT TIRE [On/Off] |  | Run-flat tire warning display status judged by the run-flat tire warning display signal received from low tire pressure warning control unit via CAN communication.
TPMS PRESS L [On/Off] |  | Low tire pressure warning display status judged by the low tire pressure warning display signal received from low tire pressure warning control unit via CAN communication.
TPMS MALF [On/Off] |  | Tire pressure monitoring system warning display status judged by the tire pressure monitoring system warning display signal received from low tire pressure warning control unit via CAN communication.
4WD CL TMP H [On/Off] |  | Display status of AWD clutch high temperature warning display signal judged by the AWD clutch high temperature warning display signal received from AWD control unit via CAN communication.
4WD TIRE CHCK [On/Off] |  | Display status of front/rear tire size discrepancy warning display judged by the front/rear tire size discrepancy warning display signal received from AWD control unit via CAN communication.
4WD SYS MALF [On/Off] |  | Display status of AWD system warning display signal judged by the AWD system warning display signal received from AWD control unit via CAN communication.
ABS MALF [On/Off] |  | Display status of anti-lock braking system (ABS) warning display judged by the ABS warning display signal received from ABS actuator and electric unit (control unit) via CAN communication.
VDC MALF [On/Off] |  | Display status of vehicle dynamic control (VDC) system warning display judged by the VDC system warning display signal received from ABS actuator and electric unit (control unit) via CAN communication.
ENG SYS CHCK [On/Off] |  | Display status of engine system warning display judged by the engine status signal received from ECM via CAN communication.
ASCD SYS MALF [On/Off] |  | Display status of cruise control system warning display judged by the ASCD status signal received from ECM via CAN communication.
ASCD REQ SPD [km] |  | ASCD set vehicle speed value that is judged by the ASCD status signal received from ECM via CAN communication.
ASCD STATUS [Off, ASCD] |  | Display status of ASCD status display judged by the ASCD status signal received from ECM via CAN communication.
ASCD SPD BLNK [On/Off] |  | Blinking status of ASCD set vehicle speed that is judged by the ASCD status signal received from ECM via CAN communication.

NOTE：
Some items are not available according to vehicle specifications.
SPECIAL FUNCTION
Special Function

Display Item | Description
W/L ON HISTORY | Lighting history of warning lamp and indicator lamp can be checked.

W/L ON HISTORY

- Stores histories when warning/indicator lamp is turned on.
- “W/L ON HISTORY” indicates the “TIME” when the warning/indicator lamp is turned on.
- The “Time” above is :

- 0: The condition that the warning/indicator lamp has been turned on 1 or more times after starting the engine and waiting for 30 seconds.
- 1 - 39: The number of times the engine was restarted after the 0 condition.
- NO W/L ON HISTORY : Stores NO (0) turning on history of warning/indicator lamp.
  NOTE：
  - W/L ON HISTORY is not stored for approximately 30 seconds after the engine starts.
  - Brake warning lamp does not store any history when the parking the brake is applied or the brake fluid level gets low.

Display Item

Display Item | Description
ABS W/L | Lighting history of ABS warning lamp.
VDC & TCS OFF W/L | Lighting history of VDC OFF indicator lamp.
SLIP IND | Lighting history of SLIP indicator lamp.
BRAKE W/L | Lighting history of brake warning lamp.
DOOR W/L | Lighting history of door open warning indication.
TRUNK/GLASS HATCH | Lighting history of trunk open warning indication.
OIL W/L | Lighting history of oil pressure warning lamp.
C-ENG W/L | Lighting history of malfunction indicator lamp (MIL).
C-ENG2 W/L | This Item is displayed, but cannot be monitored.
CRUISE IND | Lighting history of CRUISE indicator lamp.
SET IND | Lighting history of SET indicator lamp.
CRUISE W/L | This Item is displayed, but cannot be monitored.
BA W/L | This Item is displayed, but cannot be monitored.
O/D OFF IND | This Item is displayed, but cannot be monitored.
ATC/T-AMT W/L | Lighting history of transmission warning lamp.
AT OIL TEMP W/L | Lighting history of transmission oil high-temperature warning.
CVT IND | This Item is displayed, but cannot be monitored.
SPORT IND | This Item is displayed, but cannot be monitored.
4WD W/L | Lighting history of AWD warning lamp.
FUEL W/L | Lighting history of low fuel warning.
WASHER W/L | Lighting history of low washer fluid warning.
TIRE PRESS W/L | Lighting history of tire pressure warning lamp.
KEY GREEN/YELLOW IND | Lighting history of KEY warning lamp (green/yellow).
KEY RED W/L | Lighting history of KEY warning lamp (red).
KEY KNOB W/L | This Item is displayed, but cannot be monitored.
EPS W/L | This Item is displayed, but cannot be monitored.
e·4WD | This Item is displayed, but cannot be monitored.
AFS OFF IND | This Item is displayed, but cannot be monitored.
4WAS/RAS W/L | This Item is displayed, but cannot be monitored.
HDC W/L | This Item is displayed, but cannot be monitored.
SYS FAIL W/L | This Item is displayed, but cannot be monitored.
SFT POSI W/L | This Item is displayed, but cannot be monitored.
HV BAT W/L | This Item is displayed, but cannot be monitored.
HEV BRAKE W/L | This Item is displayed, but cannot be monitored.
SFT OPERATION W/L | Lighting history of shift lever position check warning.
L/K MAS W/L | This Item is displayed, but cannot be monitored.
CHARGE W/L | Lighting history of charge warning lamp.
OIL LEV LOW | Lighting history of oil level warning.
DPF W/L | This Item is displayed, but cannot be monitored.
LAUNCH CNT W/L | This Item is displayed, but cannot be monitored.