DTC DETECTION LOGIC

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2556 | PUSH-BTN IGN SW | BCM detects the push-button ignition switch stuck at ON for 100 seconds or more |

- Harness or connectors
  (Push-button ignition switch circuit is shorted.)
- Push-button ignition switch
- BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Start the engine and wait for at least 100 seconds.
2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END