REMOVAL

1.Disconnect the battery cable from the negative terminal.

2.Remove engine rear undercover, using power tools.

3.Remove harness bracket mounting bolts (A) and harness bracket.

4.Disconnect “S” connector.

5.Remove “B” terminal nut.

6.Remove starter motor mounting bolts.

7.Remove front drive shaft left side housing bolts. Refer to Exploded View (GT-R certified NISSAN dealer).

8.Move a front drive shaft left side forward keep a service area.

9.Remove starter motor (1) to left side from the vehicle.

| : Vehicle front

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
Be sure to tighten “B” terminal nut carefully.