REMOVAL

1.Remove the mounting clips, and then remove the hood insulator.

2.Remove the hood air intake mounting nuts.

3.Disengage the pawls from the hood panel.

| : Pawl

NOTE：
Press and remove the pawls from the access holes set to the panel.
■ CAUTION ■
Carefully disengage the pawls because they may be damaged if they are disengaged forcibly.

4.Slide the hood air intake (1) toward vehicle front, and then lift up and remove it from the hood panel (2).

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Securely engage the pawls with the panel until it clicks.
- Check that the guide rib does not run on to the hood panel.

  | : Guide rib