SYSTEM INITIALIZATION Perform system initialization if the following operation is performed.

- When disconnecting the battery cable and when the power supplied to the power window motor and motor is cut off by blowout of power fuse
- Removal and installation of regulator assembly
- Removal and installation of motor from regulator assembly
- Removal and installation of power window switch harness connector
- Operation of regulator assembly as an independent unit
- Removal and installation of glass
- Removal and installation of door weather-strip

Initial Setting
After installing each component, follow the steps below:

1.Disconnect the battery negative terminal or power window main switch connector. Reconnect it after waiting a minute or more.

2.Close the door.

3.Turn the ignition switch ON.

4.Operate the power window switch to fully open the glass. (This operation is unnecessary if the glass is already fully open)

5.Pull the power window switch UP (AUTO UP position). Keep pulling the switch for 2 seconds or more even after glass stops at the fully closed position.

6.Inspect anti-pinch function.
NOTE：
If the open/close operation is repeated continuously, the initial setting may be cancelled. Perform the initial setting in that situation.

CHECK ANTI-PINCH FUNCTION

1.Open the door glass fully.

2.Place a piece of wood (e.g., handle of wooden hammer) near the fully closed position.

3.Close the door glass fully with AUTO UP.

- Check that the glass lowers approximately 150 mm(5.906 in) after contacting the piece of wood and then stops. However, when the objects of more than 60 mm(2.362 in) are pinched, it is lowered approximately 100 mm(3.937 in), and then it may stop.
- Check that the glass does not rise when operating the power window main switch while lowering.

■ CAUTION ■

- Be careful not to be pinched
- Check that the auto up function is normal before the inspection following the system initialization

FITTING INSPECTION

1.Check that the overlap length with the body side weather-strip is maintained on the glass securely.

2.Check that the clearance with the side window is parallel when the glass is closed. If the clearance between glass and side window is not parallel, loosen the mounting nut of glass and carrier plate and correct the glass position.

3.Check for any unusual operation while raising and lowering the glass.

GLASS POSITION ADJUSTMENT

1.Raise glass to the fully closed position.

2.Rotate the adjustment nuts (a), (b), or (c) aligning with the upper side of glass and the body side weatherstrip to adjustment.

1. | Door glass assembly | 2. | Body side weather-strip | 3. | Body side welt (front)
4. | Front pillar finisher | 5. | Front pillar outer | 6. | Front pillar inner
7. | Roof side inner rail | 8. | Side window glass | 9. | Rear fender

NOTE：

- Basically perform the adjustment using the adjustment nut (a). Perform the adjustment using the adjustment nut (b) or (c) if the glass position is not adjusted correctly using the adjustment nut (a).
- Rotate the adjustment nut clockwise to move the door glass upper edge to the outside.
- Rotate the adjustment nut counterclockwise to move the door glass upper edge to the inside.
- Be careful that the adjustment procedure for the adjustment nut (c) is opposite in the procedure for the adjustment nut (a) or (b).