REMOVAL

1.Remove the rear seat cushion and the rear seatback. Refer to Removal and Installation.

2.Remove the kicking plate inner (LH/RH) and body side welt (LH/RH). Refer to Removal and Installation.

3.Remove the rear side finisher (LH/RH). Refer to Removal and Installation.

4.Remove the rear pillar finisher (LH/RH). Refer to Removal and Installation.

5.Remove the rear console assembly. Refer to Removal and Installation.

6.Remove the rear seat center finisher mounting bolts (B) using socket wrench (A).

7.Insert the remover tool (A) into the clearance between the rear seat center finisher (1) and the vehicle body, and then disengage the clips.

| : Clip

8.Remove the rear parcel shelf finisher mounting clips (A).

9.Remove the rear seat belt escutcheon.

10.Remove the rear seat belt inner anchor. Refer to Exploded View.

11.Disengage the child anchor cover (1) fixing pawls, with a remover tool (A) and then remove the child anchor cover (LH/RH).

12.Remove the rear seat belt (1) through the hole of rear parcel shelf finisher (2) as shown in the figure.

13.Pull and remove the rear parcel shelf finisher after disengaging the clip from the back side of rear parcel shelf finisher.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■
Check that clips are securely fitted in panel holes on body when installing the rear parcel shelf finisher and then press in.