1.CHEK MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR FUNCTION

1. Start engine.
2. Read the value indicated on boost meter in multifunction meter. Check that the value goes to negative pressure side while the engine is in idle speed, and goes to positive pressure side while the vehicle is being driven.
   ■ CAUTION ■
   Always drive vehicle at a safe speed.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Diagnosis Procedure (GT-R certified NISSAN dealer).