1.CHECK VDC OFF INDICATOR LAMP Check that the VDC OFF indicator lamp in the combination meter turns ON/OFF correctly when changing the mode to OFF mode with the set-up switch (VDC). Is the inspection result normal? YES>>GO TO 2. NO>>Replace the set-up switch (VDC). Refer to Exploded View.
2.CHECK SELF-DIAGNOSIS RESULTS
Perform self-diagnosis for “ABS” with CONSULT-III.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Perform inspection according to the displayed items.
3.CHECK COMBINATION METER
Check that the VDC OFF indicator lamp in the combination meter turns ON/OFF correctly when changing the mode to OFF mode with the set-up switch (VDC).
Is the inspection result normal?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Check the combination meter. Refer to CONSULT-III Function (METER/M&A).