■ WARNING ■

- Park the vehicle on a level surface when using the jack. Check to avoid damaging pipes, tubes, etc. under the vehicle.
- Never get under the vehicle while it is supported only by the jack. Always use safety stands when you have to get under the vehicle.
- Place wheel chocks at both front and back of the wheels on the ground.
- When lifting the vehicle, open the lift arms as wide as possible and ensure that the front and rear of the vehicle are well balanced.
- When setting the lift arm, never allow the arm to contact the brake tubes, brake cable, fuel lines and sill spoiler.

1. | Safety stand point and lift up point (front) | 2. | Safety stand point and lift up point (rear) | 3. | Garage jack point (front)
4. | Garage jack point (rear) |  |  |  |

■ CAUTION ■
There is canister just behind Garage jack point rear. Jack up carefully.