DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1708 | [NO DATA] FL | Tire pressure data signal from the front left wheel transmitter cannot be detected. |

- Harness or connector connection malfunction
  (Tire pressure receiver, low tire pressure warning control unit)
- Transmitter ID registration incomplete
- Transmitter error
- Low transmitter battery voltage

C1709 | [NO DATA] FR | Tire pressure data signal from the front right wheel transmitter cannot be detected.
C1710 | [NO DATA] RR | Tire pressure data signal from the rear right wheel transmitter cannot be detected.
C1711 | [NO DATA] RL | Tire pressure data signal from the rear left wheel transmitter cannot be detected.

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1708”, “C1709”, “C1710”, or “C1711” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END