1.CHECK THROTTLE CONTROL MOTOR

1. Turn ignition switch OFF.
2. Disconnect electric throttle control actuator harness connector.
3. Check resistance between electric throttle control actuator terminals as follows.

   Electric throttle control actuator | Resistance
   Bank | Terminals
   1 | 5 and 6 | Approx. 1 - 15 Ω [at 25°C (77°F)]
   2 | 1 and 2

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.REPLACE ELECTRIC THROTTLE CONTROL ACTUATOR

1. Replace malfunctioning electric throttle control actuator.
2. Go to Special Repair Requirement (GT-R certified NISSAN dealer).

>>INSPECTION END