NOTE： Unlock the fuel filler lid by pulling the rod if the operation of fuel filler lid opener actuator (1) is malfunctioning. REMOVAL

1.Remove the mounting screws, and then remove the fuel filler lid.

2.Push and disengage the tabs of lock and cable assembly from the vehicle body, and remove them.

3.Rotate the lock nut counterclockwise and remove it.

4.Push the tabs of fuel filler lid opener actuator, and then press them toward vehicle rear.

5.Remove the trunk side finisher lower (RH). Refer to Exploded View.

6.Disconnect the connector, and then remove the fuel filler lid opener actuator.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
After installation, check fuel filler lid open/close, lock/unlock operation.