1.CHECK COOLING FAN MOTOR

1. Turn ignition switch OFF.
2. Disconnect cooling fan control module 1 and 2 harness connectors.
3. Supply cooling fan control module 1and 2 harness connector terminals with battery voltage as per the following, and check operation.

   Cooling fan control module 1 and 2 | Operation
   Motor | Connector | Terminal
   (+) | (–)
   1 | E301 | 4 and 6 | 5 and 7 | Cooling fan operates.
   E302
   2 | E303 | 4 and 6 | 5 and 7
   E304

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace malfunctioning cooling fan motor.