WORK SUPPORT

Service item | Setting item | Description
WIPER SPEED SETTING | On | With vehicle speed (Front wiper intermittent time linked with the vehicle speed and wiper intermittent dial position)
Off* | Without vehicle speed (Front wiper intermittent time linked with the wiper intermittent dial position)
*:Factory setting

DATA MONITOR

Monitor Item [Unit] | Description
PUSH SW [Off/On] | The switch status input from push-button ignition switch.
VEHICLE SPEED 1 [km/h] | The value of the vehicle speed signal received from combination meter with CAN communication.
FR WIPER HI [Off/On] | Each switch status that BCM judges from the combination switch reading function.
FR WIPER LOW [Off/On]
FR WASHER SW [Off/On]
FR WIPER INT [Off/On]
FR WIPER STOP [Off/On] | Front wiper motor (stop position) status received from IPDM E/R with CAN communication.
INT VOLUME [1 − 7] | Each switch status that BCM judges from the combination switch reading function.

ACTIVE TEST

Test item | Operation | Description
FR WIPER | Hi | Transmits the front wiper request signal (HI) to IPDM E/R with CAN communication to operate the front wiper HI operation.
Lo | Transmits the front wiper request signal (LO) to IPDM E/R with CAN communication to operate the front wiper LO operation.
INT | Transmits the front wiper request signal (INT) to IPDM E/R with CAN communication to operate the front wiper INT operation.
Off | Stops transmitting the front wiper request signal to stop the front wiper operation.