1.Remove filler plug (1). Fill up with new gear oil until oil level reaches the specified level (A).

Oil grade and Viscosity | : Refer to Fluids and Lubricants.
Oil capacity | : Refer to General Specifications.

2.After refilling oil, check oil level. Set a gasket to filler plug (1), and then install it to final drive and tighten to the specified torque. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■
Never reuse gasket.