1.CHECK INTAKE AIR TEMPERATURE SENSOR

1. Turn ignition switch OFF.
2. Disconnect mass air flow sensor (bank 1) harness connector.
3. Check resistance between mass air flow sensor (bank 1) terminals as follows.

   Terminals | Condition | Resistance (kΩ)
   1 and 2 | Temperature [°C (°F)] | 25 (77) | 1.800 - 2.200

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace mass air flow sensor (with intake air temperature sensor) (bank 1).