1.CHECK TRUNK LID OPENER REQUEST SWITCH

1. Turn ignition switch OFF.
2. Disconnect trunk lid opener request switch connector.
3. Check continuity between trunk lid opener request switch terminals.

Trunk lid opener request switch | Condition | Continuity
Terminal
1 | 2 | Trunk lid opener request switch | Pressed | Existed
Released | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace trunk lid opener request switch. Refer to Removal and Installation.