DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible causes
P2734 | Pressure control solenoid "F" electrical | A DTC is set if the line pressure solenoid valve monitor current value is less than 0.2 A when the line pressure solenoid valve target current value is more than 0.38 A. |

- Line pressure solenoid valve
- Harness or connector
  (Open or short in the line pressure solenoid valve circuit)

DTC CONFIRMATION PROCEDURE
■ CAUTION ■
Be careful of the driving speed.
1.PREPARATION BEFORE OPERATION (PART 1)
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PREPARATION BEFORE OPERATION (PART 2)
With CONSULT-III

1. Turn the ignition switch ON.
2. Select “FLUID TEMP” in “Data Monitor”.

Without CONSULT-III

1. Turn the ignition switch ON.
2. Check “TRANS OIL TEMP” on multi-function display.

Is the oil temperature 30°C (86°F) or more?
YES>>GO TO 3.
NO>>Warm up the transmission.
3.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Shift the shift lever to the N position.
   ■ CAUTION ■
   No shift position indicator in the combination meter blinks.
2. Start the engine.
3. With the shift lever in the N position, and run at idle for 5 seconds or more.
4. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Shift the shift lever to the N position.
   ■ CAUTION ■
   No shift position indicator in the combination meter blinks.
2. Start the engine.
3. With the shift lever in the N position, and run at idle for 5 seconds or more.
4. Check self-diagnosis.

Is DTC P2734 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.