1.CHECK GROUND CONNECTION

1. Turn ignition switch OFF.
2. Check ground connection M95. Refer to Ground Inspection in Circuit Inspection.

Is the inspection result normal?
YES>>GO TO 2.
NO>>Repair or replace ground connection.
2.CHECK EVAP CONTROL SYSTEM PRESSURE SENSOR CONNECTOR FOR WATER

1. Disconnect EVAP control system pressure sensor harness connector.
2. Check that water is not inside connectors.

Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace harness connector.
3.CHECK EVAP CONTROL SYSTEM PRESSURE SENSOR
Refer to Component Inspection (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>GO TO 4.
NO>>Replace EVAP control system pressure sensor.
4.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END