INSPECTION AFTER REMOVAL Appearance Check the following items, and replace the part if necessary.

- Rear lower link for deformation, cracks or damage.
- Axle housing side bushing boots for cracks, damage or leakage of grease.
  NOTE：
  Pillow ball bushing to axle housing side of rear lower link.

Pillow ball bushing Inspection
Manually move pillow ball bushing to check that it moves smoothly with no binding and check for looseness. Replace the rear lower link if necessary.
INSPECTION AFTER INSTALLATION

1.Check wheel alignment. Refer to Inspection.

2.Adjust neutral position of steering angle sensor. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).