DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1144 | ST ANG SEN SIGNAL | Adjustment of steering angle sensor neutral position is not finished. |

- Steering angle sensor
- ABS actuator and electric unit (control unit)

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Turn the ignition switch ON.
2. Perform adjust the neutral position of steering angle sensor. Refer to Description (GT-R certified NISSAN dealer).
3. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1144” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END