1.VDC OFF INDICATOR LAMP OPERATION CHECK 1 Check that the lamp illuminates for approximately 2 second after the ignition switch is turned ON. Is the inspection result normal? YES>>GO TO 2. NO>>Check combination meter. Refer to CONSULT-III Function (METER/M&A).
2.VDC OFF INDICATOR LAMP OPERATION CHECK 2
Check that the VDC OFF indicator lamp in the combination meter turns ON/OFF correctly when changing the mode to OFF mode with the set-up switch (VDC).
Is the inspection result normal?
YES>>INSPECTION END
NO>>Check VDC OFF switch. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).