DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P2715 | Pressure control solenoid "D" stuck on |

- A DTC is set if the clutch B pressure sensor value is less than 0.4 MPa (4.08 kg/cm2, 58 psi) when the axis B feed pressure target value is 0.4 MPa (4.08 kg/cm2, 58 psi) or more.
- A DTC is set if the clutch B pressure sensor value is more than 0.2 MPa (2.04 kg/cm2, 29 psi) when the axis B feed pressure target value is 0.1 MPa (1.02 kg/cm2, 14.5 psi) or less.

- Axis B feed pressure solenoid valve
- Clutch B solenoid valve
- Clutch B pressure sensor
- Clutch B oil passage
- Harness or connector
  (Open or short in the axis B feed pressure solenoid valve circuit)
  (Open or short in the clutch B solenoid valve circuit)
  (Open or short in the clutch B pressure sensor circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn the ignition switch ON.
2. Shift the shift lever to the P position.
3. Start the engine.
4. With the shift lever in the P position, and run at idle for 1 minute or more.
5. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn the ignition switch ON.
2. Shift the shift lever to the P position.
3. Start the engine.
4. With the shift lever in the P position, and run at idle for 1 minute or more.
5. Check self-diagnosis.

Is DTC P2715 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.