1.CHECK STOP LAMP SWITCH-I

1. Turn ignition switch OFF.
2. Disconnect stop lamp switch harness connector.
3. Check the continuity between stop lamp switch terminals under the following conditions.

   Terminals | Condition | Continuity
   1 and 2 | Brake pedal | Fully released | Not existed
   Slightly depressed | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.CHECK STOP LAMP SWITCH-II

1. Adjust stop lamp switch installation. Refer to Inspection and Adjustment.
2. Check the continuity between stop lamp switch terminals under the following conditions.

   Terminals | Condition | Continuity
   1 and 2 | Brake pedal | Fully released | Not existed
   Slightly depressed | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace stop lamp switch.