1.CHECK TRUNK LID OPENER SWITCH Check trunk lid opener switch. Refer to Component Function Check. Is the inspection result normal? YES>>GO TO 2.
NO>>Repair or replace the malfunctioning parts.
2.CHECK TRUNK LID OPENER ACTUATOR
Check trunk lid opener actuator.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK TRUNK LID OPENER CANCEL SWITCH
Check trunk lid opener cancel switch.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.CHECK VEHICLE SPEED SIGNAL
Check combination meter.
Refer to DTC Index.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.