PROPELLER SHAFT RUNOUT Check propeller shaft runout at measuring point with a dial indicator. If runout exceeds specifications, replace propeller shaft assembly. For measuring point, refer to Inspection (GT-R certified NISSAN dealer).

Limit
Propeller shaft runout | : Refer to Propeller Shaft Runout (GT-R certified NISSAN dealer).

JOURNAL AXIAL PLAY

- As shown in the figure, while fixing yoke on one side, check axial play of joint. If it is outside the standard, replace propeller shaft assembly.

  Standard
  Journal axial play | : Refer to Journal Axial Play (GT-R certified NISSAN dealer).

■ CAUTION ■
Never disassemble joints.
CENTER BEARING
Check center bearing for noise and damage. If noise or damage is detected, replace propeller shaft assembly.
■ CAUTION ■
Never disassemble center bearing.