1.PERFORM PRESSURE SENSOR CALIBRATION Perform the pressure sensor calibration. Refer to Special Repair Requirement (GT-R certified NISSAN dealer). Is pressure sensor calibration completed? YES>>INSPECTION END NO>>GO TO 2.
2.CHECK PRESSURE SENSOR
Check pressure sensor. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Repair or replace error-detected parts.