When TCM is replaced, learning must be performed. ■ CAUTION ■

- Before TCM is replaced, it is necessary to acquire the IP characteristic data based on the information read out from the malfunctioning TCM. For acquiring the IP characteristic data, refer to “CONSULT-III GT-R TCM CONFIGURATION MANUAL”.
- If no IP characteristic data can be acquired, it is necessary to replace TCM and the transmission assembly as a set.